1. **Board of Forestry and Fire Protection**
2. **Tractor Operations and Cable Yarding Amendments, 2023**
3. **Title 14 of the California Code of Regulations**
4. **Division 1.5, Chapter 4,**
5. **Subchapter 1, Article 1;**
6. **Subchapters 4, 5, & 6, Article 4;**

7

1. **§ 914.2. Operations.**
2. (a) Timber Operations shall be conducted in a manner which complies with 14 CCR §
3. 914.
4. (b) Heavy equipment which is equipped with a blade, shall not operate on skid roads or
5. slopes that are so steep as to require the use of the blade for braking.
6. (c) Tractor Roads shall be limited in number and width to the minimum necessary for
7. removal of logs.
8. (d) Heavy equipment shall not operate on Unstable Areas. If such areas are
9. unavoidable, the RPF shall develop specific measures to minimize the effect of
10. operations on slope instability. These measures shall be explained and justified in the
11. Plan and approved by the Director, and must meet the requirements of 14 CCR § 914.
12. (e) Slash and debris from Timber Operations shall not be bunched adjacent to residual
13. trees required for silvicultural or wildlife purposes or placed in locations where they
14. could be discharged into a Class I or II Watercourse, or Lake.
15. (f) The following limitations apply:
16. (1) Except for Tethered Operations, heavy equipment shall be prohibited where any of
17. the following conditions are present:
18. (A) Slopes steeper than 65%
19. (B) Slopes steeper than 50% where the Erosion Hazard Rating is high or extreme
20. (2) Heavy equipment shall be prohibited on slopes over 50% which lead without
21. flattening to sufficiently dissipate water flow and trap sediment before it reaches a
22. Watercourse or Lake.
23. (3) On slopes between fifty (50) percent and sixty-five (65) percent where the Erosion
24. Hazard Rating is moderate, and all slope percentages are for Average Slope steepness
25. based on sample areas that are twenty (20) acres, or less if proposed by the RPF or
26. required by the Director, heavy equipment, except for Tethered Operations, shall be
27. limited to:
28. (A) existing Tractor Roads that do not require reconstruction, or
29. (B) New Tractor Roads at a location that has been shown on the Plan map, flagged by
30. an RPF or Supervised Designee prior to the pre-harvest inspection or, when a pre-
31. harvest inspection is not required, prior to the start of Timber Operations, and approved
32. by the Director.
33. (4) ~~The RPF may propose exceptions to the limitations on Tractor Operations described~~
34. ~~above if the proposed exception will comply with 14 CCR § 914, and if the Plan both~~
35. ~~clearly explains the proposed exception and justifies how the proposed exception will~~
36. ~~comply with 14 CCR § 914. The location of Tractor Roads, except for those used in~~
37. ~~Tethered Operations, to be used under such exceptions shall be flagged prior to the~~
38. ~~pre-harvest inspection or, when a pre-harvest inspection is not required, prior to the~~
39. ~~start of Timber Operations.~~
40. ~~(5)~~ Non-Tethered Tractor Operations, excluding Yarding, may occur in areas designated
41. for Cable Yarding on slopes up to 50%. Tethered Operations, excluding Yarding, may
42. occur in areas designated for Cable Yarding. The limitations of 14 CCR § 914.2(a), (b),
43. (c), (d), (e), (f)(2), (g), (h), and (i), and any other applicable limitations on Tractor
44. Operations throughout this Chapter, by District, apply.
45. (5) The RPF may propose exceptions to the limitations on Tractor Operations described
46. above if the proposed exception will comply with 14 CCR § 914, and if the Plan both
47. clearly explains the proposed exception and justifies how the proposed exception will
48. comply with 14 CCR § 914. The location of Tractor Roads, except for those used in
49. Tethered Operations, to be used under such exceptions shall be flagged prior to the
50. pre-harvest inspection or, when a pre-harvest inspection is not required, prior to the
51. start of Timber Operations.
52. (g) Where Tractor Roads are constructed, Timber Operators shall use Tractor Roads
53. only, both for Skidding logs to Landings and on return trips.
54. (h) Timber Operators shall exercise due diligence so that desirable residual trees and
55. seedlings which are required to be retained upon completion of Timber Operations will
56. not be damaged or destroyed by Timber Operations.
57. (i) Where Waterbreaks cannot effectively disperse surface runoff, other Erosion
58. Controls shall be installed as needed.

17

1. NOTE: Authority cited: Sections 4551, 4551.5 and 4553, Public Resources Code.
2. Reference: Sections 4512, 4513, 4562.5, 4562.7 and 4582, Public Resources Code.

20

21 \*\*\*\*\*

22

1. **§ 934.2. Operations.**
2. (a) Timber Operations shall be conducted in a manner which complies with 14 CCR §
3. 934.
4. (b) Heavy equipment which is equipped with a blade, shall not operate on skid roads or
5. slopes that are so steep as to require the use of the blade for braking.
6. (c) Tractor Roads shall be limited in number and width to the minimum necessary for
7. removal of logs. The RPF may propose exceptions for silvicultural reasons when
8. explained and justified in the Plan.
9. (d) Heavy equipment shall not operate on Unstable Areas. If such areas are
10. unavoidable, the RPF shall develop specific measures to minimize the effect of
11. operations on slope instability. These measures shall be explained and justified in the
12. Plan and approved by the Director, and must meet the requirements of 14 CCR § 934.
13. (e) Slash and debris from Timber Operations shall not be bunched adjacent to residual
14. trees required for silvicultural or wildlife purposes or placed in locations where they
15. could be discharged into a Class I or II Watercourse, or Lake.
16. (f) The following limitations apply:
17. (1) Except for Tethered Operations, heavy equipment shall be prohibited where any of
18. the following conditions are present:
19. (A) Slopes steeper than 65%
20. (B) Slopes steeper than 50% where the Erosion Hazard Rating is high or extreme
21. (2) Heavy equipment shall be prohibited on slopes over 50% which lead without
22. flattening to sufficiently dissipate water flow and trap sediment before it reaches a
23. Watercourse or Lake.
24. (3) On slopes between fifty (50) percent and sixty-five (65) percent where the Erosion
25. Hazard Rating is moderate, and all slope percentages are for Average Slope steepness
26. based on sample areas that are twenty (20) acres, or less if proposed by the RPF or
27. required by the Director, heavy equipment, except for Tethered Operations, shall be
28. limited to:
29. (A) existing Tractor Roads that do not require reconstruction, or
30. (B) New Tractor Roads at a location that has been shown on the Plan map, flagged by
31. an RPF or Supervised Designee prior to the pre-harvest inspection or, when a pre-
32. harvest inspection is not required, prior to the start of Timber Operations, and approved
33. by the Director.
34. (4) ~~The RPF may propose exceptions to the limitations on Tractor Operations described~~
35. ~~above if the proposed exception will comply with 14 CCR § 934, and if the Plan both~~
36. ~~clearly explains the proposed exception and justifies how the proposed exception will~~
37. ~~comply with 14 CCR § 934. The location of Tractor Roads, except for those used in~~
38. ~~Tethered Operations, to be used under such exceptions shall be flagged prior to the~~
39. ~~pre-harvest inspection or, when a pre-harvest inspection is not required, prior to the~~
40. ~~start of Timber Operations.~~
41. ~~(5)~~ Non-Tethered Tractor Operations, excluding Yarding, may occur in areas designated
42. for Cable Yarding on slopes up to 50%. Tethered Operations, excluding Yarding, may
43. occur in areas designated for Cable Yarding. The limitations of 14 CCR § 934.2(a), (b),
44. (c), (d), (e), (f)(2), (g), (h), and (i), and any other applicable limitations on Tractor
45. Operations throughout this Chapter, by District, apply.
46. (5) The RPF may propose exceptions to the limitations on Tractor Operations described
47. above if the proposed exception will comply with 14 CCR § 934, and if the Plan both
48. clearly explains the proposed exception and justifies how the proposed exception will
49. comply with 14 CCR § 934. The location of Tractor Roads, except for those used in
50. Tethered Operations, to be used under such exceptions shall be flagged prior to the
51. pre-harvest inspection or, when a pre-harvest inspection is not required, prior to the
52. start of Timber Operations.
53. (g) Where Tractor Roads are constructed, Timber Operators shall use Tractor Roads
54. only, both for Skidding logs to Landings and on return trips.
55. (h) Timber Operators shall exercise due diligence so that desirable residual trees and
56. seedlings which are required to be retained upon completion of Timber Operations will
57. not be damaged or destroyed by Timber Operations.
58. (i) Where Waterbreaks cannot effectively disperse surface runoff, other Erosion
59. Controls shall be installed as needed.

8

1. NOTE: Authority cited: Sections 4551, 4551.5 and 4553, Public Resources Code.
2. Reference: Sections 4512, 4513, 4562.5, 4562.7 and 4582, Public Resources Code.

11

12 \*\*\*\*\*\*

13

1. **§ 954.2. Operations.**
2. (a) Timber Operations shall be conducted in a manner which complies with 14 CCR §
3. 954.
4. (b) Heavy equipment which is equipped with a blade, shall not operate on skid roads or
5. slopes that are so steep as to require the use of the blade for braking.
6. (c) Tractor Roads shall be limited in number and width to the minimum necessary for
7. removal of logs.
8. (d) Heavy equipment shall not operate on Unstable Areas. If such areas are
9. unavoidable, the RPF shall develop specific measures to minimize the effect of
10. operations on slope instability. These measures shall be explained and justified in the
11. Plan and approved by the Director, and must meet the requirements of 14 CCR § 954.
12. (e) Slash and debris from Timber Operations shall not be bunched adjacent to residual
13. trees required for silvicultural or wildlife purposes or placed in locations where they
14. could be discharged into a Class I or II Watercourse, or Lake.
15. (f) The following limitations apply:
16. (1) Except for Tethered Operations, heavy equipment shall be prohibited where any of
17. the following conditions are present:
18. (A) Slopes steeper than 65%
19. (B) Slopes steeper than 50% where the Erosion Hazard Rating is high or extreme
20. (2) Heavy equipment shall be prohibited on slopes over 50% which lead without
21. flattening to sufficiently dissipate water flow and trap sediment before it reaches a
22. Watercourse or Lake.
23. (3) On slopes between fifty (50) percent and sixty-five (65) percent where the Erosion
24. Hazard Rating is moderate, and all slope percentages are for Average Slope steepness
25. based on sample areas that are twenty (20) acres, or less if proposed by the RPF or
26. required by the Director, heavy equipment, except for Tethered Operations, shall be
27. limited to:
28. (A) existing Tractor Roads that do not require reconstruction, or
29. (B) New Tractor Roads at a location that has been shown on the Plan map, flagged by
30. an RPF or Supervised Designee prior to the pre-harvest inspection or, when a pre-
31. harvest inspection is not required, prior to the start of Timber Operations, and approved
32. by the Director.
33. (4) ~~The RPF may propose exceptions to the limitations on Tractor Operations described~~
34. ~~above if the proposed exception will comply with 14 CCR § 954, and if the Plan both~~
35. ~~clearly explains the proposed exception and justifies how the proposed exception will~~
36. ~~comply with 14 CCR § 954. The location of Tractor Roads, except for those used in~~
37. ~~Tethered Operations, to be used under such exceptions shall be flagged prior to the~~
38. ~~pre-harvest inspection or, when a pre-harvest inspection is not required, prior to the~~
39. ~~start of Timber Operations.~~
40. ~~(5)~~ Non-Tethered Tractor Operations, excluding Yarding, may occur in areas designated
41. for Cable Yarding on slopes up to 50%. Tethered Operations, excluding Yarding, may
42. occur in areas designated for Cable Yarding. The limitations of 14 CCR § 914.2(a), (b),
43. (c), (d), (e), (f)(2), (g), (h), and (i), and any other applicable limitations on Tractor
44. Operations throughout this Chapter, by District, apply.
45. (5) The RPF may propose exceptions to the limitations on Tractor Operations described
46. above if the proposed exception will comply with 14 CCR § 954, and if the Plan both
47. clearly explains the proposed exception and justifies how the proposed exception will
48. comply with 14 CCR § 954. The location of Tractor Roads, except for those used in
49. Tethered Operations, to be used under such exceptions shall be flagged prior to the
50. pre-harvest inspection or, when a pre-harvest inspection is not required, prior to the
51. start of Timber Operations.
52. (g) Where Tractor Roads are constructed, Timber Operators shall use Tractor Roads
53. only, both for Skidding logs to Landings and on return trips.
54. (h) Timber Operators shall exercise due diligence so that desirable residual trees and
55. seedlings which are required to be retained upon completion of Timber Operations will
56. not be damaged or destroyed by Timber Operations.
57. (i) Where Waterbreaks cannot effectively disperse surface runoff, other Erosion
58. Controls shall be installed as needed.

23

1. NOTE: Authority cited: Sections 4551, 4551.5 and 4553, Public Resources Code.
2. Reference: Sections 4512, 4513, 4562.5, 4562.7 and 4582, Public Resources Code.