**Board of Forestry and Fire Protection**

**Ford Definition Amendment, 2023**

**Title 14 of the California Code of Regulations**

**Division 1.5, Chapter 4,**

**Subchapter 1**

**OPTION #1**

\*\*\*\*\*

**§ 895.1. Definitions**

**Ford** means a Logging Road Watercourse crossing where the road grade dips through the natural grade of the Watercourse channel where no fill is placed within the channel.

**Rock-armored crossing** means a Logging Road Watercourse crossing where fill is placed in the channel to establish a usable road grade and the outfall of the crossing and road surface are protected against scour by revetment composed of rock.

**Rock-fill crossing** means a Logging Road Watercourse crossing where rock that is free of fines is placed as fill in the channel to establish a usable road grade through the crossing.

**Vented crossing** means a Logging Road Watercourse crossing designed to allow low water flow in the stream channel to pass through the structure, usually through a culvert, below a hardened roadway, and high water flow to pass over the roadway.

\*\*\*\*\*

**OPTION #2**

\*\*\*\*\*

**§ 895.1. Definitions**

**Ford** means a Logging Road Watercourse crossing where the road grade dips through the Watercourse channel, including native surface, rock, armored fill, and vented.

\*\*\*\*\*